INSTRUMENT CLUSTER SPECIFICATIONS

id092200101100

Item | Specification
--- | ---
Speedometer | Meter type | Stepping motor type
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Tachometer | Meter type | Stepping motor type
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Fuel gauge | Meter type | Stepping motor type (Reset-to-zero type)
Input signal communication system | Conventional communication system
Input signal source | • Fuel gauge sender unit (Main) • Fuel gauge sender unit (Sub)
Rated voltage | (V) | DC 12
Water temperature gauge | Meter type | Stepping motor type (Medium range stabilized type)
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
Odometer/Tripmeter | Display | LCD
Indication digits | Odometer: 6 digits, Tripmeter: 4 digits
Input signal communication system | CAN system
Input signal source | PCM
Rated voltage | (V) | DC 12
FOW/LDWS display (with FSC) | Display | LCD
Input signal communication system | CAN system
Input signal source | Forward sensing camera (FSC)
Rated voltage | (V) | DC 12
Warning/indicator alarms
Sound frequency | (Hz) | 1,000—2,200
Output sound pressure level | (dB) | 51.0—77.0
Lights-on reminder warning alarm | Sound frequency | (Hz) | 1,900
Sound cycle |
Key reminder warning alarm | Sound frequency | (Hz) | 1,800
Sound cycle |
Seat belt warning alarm | Sound frequency | (Hz) | 1,000
Sound cycle |
Advanced keyless entry system warning alarm | Sound frequency | (Hz) | 1,800
Sound cycle |
Air bag system warning alarm | Sound frequency | (Hz) | 2,200
Sound cycle |
Parking brake reminder warning alarm | Sound frequency | (Hz) | 2,000
Sound cycle |
BSM warning alarm (RCTA warning alarm ) | Sound frequency | (Hz) | 2,000
Sound cycle |
LDWS warning alarm | Sound frequency | (Hz) | 2,000
Sound cycle |
FOW warning alarm | Sound frequency | (Hz) | 2,000
Sound cycle |
Turn and hazard indicator alarm | Sound frequency | (Hz) | 1,700—1,800
Sound cycle |
Panel light control indicator alarm | Sound frequency | (Hz) | 1,900
Sound cycle |

Information Display

Item | Specification
--- | ---
Clock accuracy (Reference value)* | (s/day) | -1.5—1.5

* :If the clock accuracy varies largely from the reference value, battery deterioration or an information display malfunction may have occurred.