REAR TILT MOTOR INSPECTION

id091300800800

1. Disconnect the rear tilt motor connector.

2. Apply battery positive voltage to the rear tilt motor terminals and inspect the rear tilt motor operation

ac9wzw00001243

  • If not as specified, replace the slide adjuster. (See FRONT SEAT SLIDE ADJUSTER REMOVAL/INSTALLATION.)

Motor operation | Connection
--- | ---
B+ | GND
Up | D | E
Down | E | D

3. Connect the rear tilt motor connector.

4. Measure the rear tilt motor terminal A waveform during motor operation using the oscilloscope.

Condition | Voltage (V)
--- | ---
High output | 4.8 or more
Low output | 1.0 or less

• If not as specified, replace the slide adjuster. (See FRONT SEAT SLIDE ADJUSTER REMOVAL/INSTALLATION.)