REAR EVAPORATOR TEMPERATURE SENSOR REMOVAL/INSTALLATION

id074000804400

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (6) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (7) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (8) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (9) Console (See CONSOLE REMOVAL/INSTALLATION.)

3. Disconnect the rear evaporator temperature sensor connector and remove it from the rear A/C unit.

ac9wzw00002806

4. Insert a flathead screwdriver as shown in the figure and remove the clip by prying it off.

5. Remove the rear evaporator temperature sensor.

6. Install in the reverse order of removal.