KEYLESS CONTROL MODULE REMOVAL/INSTALLATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008063z6

  Note
  • If the keyless control module is replaced, always perform the following procedure.
  Without immobilizer system
    ― Keyless control module configuration (See KEYLESS CONTROL MODULE CONFIGURATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
    ― Advanced key programming (See CLEARING ADVANCED KEY [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
    ― Steering lock unit programming (See STEERING LOCK UNIT ID CODE REGISTRATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
  With immobilizer system
    ― Keyless control module configuration (See KEYLESS CONTROL MODULE CONFIGURATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
    ― Advanced key programming (See CLEARING ADVANCED KEY [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
    ― Steering lock unit programming (See STEERING LOCK UNIT ID CODE REGISTRATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
    ― Immobilizer system resetting (with immobilizer system) (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [KEYLESS ENTRY SYSTEM].) (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [KEYLESS ENTRY SYSTEM].)

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the auto light/wiper control module. (Vehicles with auto light/wiper system) (See AUTO LIGHT/WIPER CONTROL MODULE REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00002974

1 | Connector
2 | Screw
3 | Keyless control module

5. Install in the reverse order of removal.