FRONT AIRFLOW MODE ACTUATOR INSPECTION

id074000804500

1. Connect battery positive voltage to front airflow mode actuator terminal F (or G), connect terminal G (or F) to ground, and then verify that the front airflow mode actuator operates as shown in the table.

  • If the operation condition is not normal, replace the front airflow mode actuator.

ac9wzw00002807

Terminal | Front airflow mode actuator operation
--- | ---
F | G
B+ | Ground | VENT → DEFROSTER
Ground | B+ | DEFROSTER → VENT

am8rrw00000825

2. Verify that the resistance between terminals C and E, and E and A matches the front airflow mode actuator operation as shown in the graph.

am8rrw00000826

  • If the operation condition and resistance are not normal, replace the front airflow mode actuator.