REAR WIPER MOTOR INSPECTION

id091900801500

1. Connect battery positive voltage to the rear wiper motor terminal A, and ground the rear wiper motor terminal B.

2. Verify that the rear wiper motor operates.

ac9wzw00001597

  • If there is any malfunction, replace the rear wiper motor. (See REAR WIPER MOTOR REMOVAL/INSTALLATION.)

3. Disconnect the ground to the terminal B while the rear wiper is operating.

4. Verify that the rear wiper stops in the park position.

  • If there is any malfunction, replace the rear wiper motor. (See REAR WIPER MOTOR REMOVAL/INSTALLATION.)