POSITIVE CRANKCASE VENTILATION (PCV) VALVE REMOVAL/INSTALLATION [MZI-3.7]

id0116d2819800

  Caution
  • A new PCV valve must be installed if removed from the cylinder head cover.
  • Upon removal, damage will occur to the locking mechanism on the PCV valve.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove in the order indicated in the table.

ac9wzw00002194

1 | PCV valve hose
2 | PCV valve
3 | O-ring

3. Install in the reverse order of removal.