RADIATOR GRILLE REMOVAL/INSTALLATION

id091600800900

1. Set the front over fender out of the way. (See OVER FENDER REMOVAL/INSTALLATION.)

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the radiator grille. (See FRONT BUMPER DISASSEMBLY/ASSEMBLY.)

4. Disassemble in the order indicated in the table.

ac9wzw00003009

1 | Fastener
2 | Screw A
3 | Clip
4 | Grille bracket
5 | Screw B
6 | Garnish
7 | Screw C
8 | Lower radiator grille
9 | Ornament
10 | Rivet
11 | Upper radiator grille
12 | Radiator grille reinforcement

5. Assemble in the reverse order of disassembly.