FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION

id091700809600

1. Insert a tape-wrapped flathead screwdriver between the indicator panel and front console box mat.

ac9uuw00002134

  Caution
  • The rubber may deform if it is pried with a flathead screwdriver. Therefore, fully insert a tape-wrapped flathead screwdriver as shown in the figure, and do not pry the rubber.

2. Raise the front console box mat.

3. Remove the front console box mat in the direction of the arrow.

ac9uuw00000576

4. Remove the front console box mat.

5. Install in the reverse order of removal.