FAN MOTOR INSPECTION [MZI-3.7]

id0112d3800900

Part Inspection

1. Verify that the battery is fully charged. (See BATTERY INSPECTION [MZI-3.7].)

2. Disconnect the cooling fan motor connector (fan control module side, 2 terminals).

3. Install a tester and battery to the cooling fan motor connector as shown in the figure.

ac9wzw00002178

4. Verify that each fan motors operate smoothly at the standard current.

  • If there is any malfunction, replace the applicable part.

  Cooling fan motor standard current

  No.1, No.2: 17—23 A [12 V]