FRONT MAP LIGHT REMOVAL/INSTALLATION

id091800808000

1. Disconnect the negative battery cable.

2. Remove the intruder sensor. (with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00001784

1 | Lens (See Lens Removal Note.)
2 | Screw
3 | Front map light bulb
4 | Front map light
5 | Connector

4. Install in the reverse order of removal.

Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole and pry with the screwdriver in the direction shown by the arrow to remove the lens.

ac9uuw00000791