DTC TABLE [BCM]

id0902f5347100

DTC No. | Detection condition | Description | Page
--- | --- | --- | ---
B1317 | • BCM power supply voltage from the battery is 16 V or more. | BCM power supply voltage high input | (See DTC B1317 [BCM].)
B1318 | • BCM power supply voltage from the battery is less than 9 V. | BCM power supply voltage low input | (See DTC B1318 [BCM].)
B1322 | • Short to ground in front door switch (driver-side) circuit with the front door (driver-side) closed (front door switch (driver-side) off). | Front door switch (driver-side) circuit malfunction | (See DTC B1322 [BCM].)
B1330 | • Short to ground in front door switch (passenger-side) circuit with the front door (passenger-side) closed (front door switch (passenger-side) off). | Front door switch (passenger-side) circuit malfunction | (See DTC B1330 [BCM].)
B1342 | • BCM detects the internal ECU malfunction. | BCM internal ECU malfunction | (See DTC B1342 [BCM].)
B1502 | • Short to ground in turn switch (LH) circuit with the turn switch off. | Turn switch (LH) circuit malfunction | (See DTC B1502 [BCM].)
B1506 | • Short to ground in turn switch (RH) circuit with the turn switch off. | Turn switch (RH) circuit malfunction | (See DTC B1506 [BCM].)
B1520*1 | • Open circuit in bonnet latch switch circuit with the bonnet closed (bonnet latch switch on). | Bonnet latch switch circuit malfunction | (See DTC B1520 [BCM].)
B1566 | • Short to ground in rear door switch (LH) or (RH) circuit with the rear doors closed (rear door switches off). | Rear door switch (LH)/(RH) circuit malfunction | (See DTC B1566 [BCM].)
B1614 | • Short to ground in rear wiper INT switch circuit with the rear wiper switch off. | Rear wiper INT switch circuit malfunction | (See DTC B1614 [BCM].)
B1873 | • Short to ground in hazard warning switch circuit with the hazard warning switch off. | Hazard warning switch circuit malfunction | (See DTC B1873 [BCM].)
B2218 | • Door lock switch (driver-side) or (passenger-side) circuit voltage is less than 3.75 V with the door lock switches off. | Door lock switch (driver-side)/(passenger-side) circuit malfunction | (See DTC B2218 [BCM].)
B2574 | • Short to ground in front door lock-link switch (driver-side) lock-side circuit with the front door lock-link switch (driver-side) unlocked. | Front door lock-link switch (driver-side) lock-side circuit malfunction | (See DTC B2574 [BCM].)
B257C*1 | • Open circuit in front door lock-link switch (passenger-side), rear door lock-link switch (LH) or (RH) circuit with the door lock-link switches unlocked. | Front door lock-link switch (passenger-side)/rear door lock-link switch (LH)/(RH) circuit malfunction | (See DTC B257C [BCM].)
B2721 | • Short to ground in liftgate latch switch circuit with the liftgate closed (liftgate latch switch off). | Liftgate latch switch circuit malfunction | (See DTC B2721 [BCM].)
B2982 | • Open circuit in parking brake switch circuit with the parking brake lever pulled (parking brake switch on). | Parking brake switch circuit malfunction | (See DTC B2982 [BCM].)
C1189 | • Short to ground in brake fluid level sensor circuit with the brake fluid level on the upper side of the MIN. | Brake fluid level sensor circuit malfunction | (See DTC C1189 [BCM].)
C1295 | • BCM detects the steering angle sensor internal abnormality (signal overflow). | Steering angle sensor internal malfunction | (See DTC C1295, C1307, C1441, C1442, C1443, C1444, C144A, C144B, C144C, C144D [BCM].)
C1307 | • BCM detects the steering angle sensor internal abnormality (signal jump). | Steering angle sensor encoder ring defective
C1441 | • Open circuit in steering angle sensor A signal circuit. | Steering angle sensor A signal circuit malfunction
C1442 | • Open circuit in steering angle sensor B signal circuit. | Steering angle sensor B signal circuit malfunction
C1443 | • Short to ground in steering angle sensor A signal circuit. | Steering angle sensor A signal circuit malfunction
C1444 | • Short to ground in steering angle sensor B signal circuit. | Steering angle sensor B signal circuit malfunction
C144A | • Short to ground in steering angle sensor C signal circuit. | Steering angle sensor C signal circuit malfunction
C144B | • Short to ground in steering angle sensor Z signal circuit. | Steering angle sensor Z signal circuit malfunction
C144C | • Open circuit in steering angle sensor C signal circuit. | Steering angle sensor C signal circuit malfunction
C144D | • Open circuit in steering angle sensor Z signal circuit. | Steering angle sensor Z signal circuit malfunction
C1937 | • BCM lost the steering angle initialization position. | Steering angle sensor offset failure | (See DTC C1937 [BCM].)
U0073 | • BCM detects a CAN bus communication line (HS-CAN) malfunction. | Module communication error (HS-CAN) | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100 | • BCM cannot receive the CAN signal from the PCM for 5 s or more. | Communication error with PCM
U0101 | • BCM cannot receive the CAN signal from the TCM for 5 s or more. | Communication error with TCM
U0121 | • BCM cannot receive the CAN signal from the DSC/RSC HU/CM for 5 s or more. | Communication error with DSC/RSC HU/CM
U0401 | • BCM receives the invalid data from the PCM for 5 s or more. | Error signal from PCM | (See DTC U0401 [BCM].)

*1 :Vehicles with theft-deterrent system