REAR AIRFLOW MODE ACTUATOR CONSTRUCTION

id074000105300

Construction

• Opens/closes the mode door based on the signals from the front climate control unit to switch the air vents.
• A potentiometer type, which allows minute and smooth changes of the door position, has been adopted.

Operation

• The front climate control unit compares the voltage detected by the potentiometer in the rear airflow actuator with the target voltage.
• Operates the motor in the rear airflow actuator until the detected voltage and the target voltage are equal.

ac9wzn00000865