AUTOMATIC TRANSAXLE FLUID (ATF) LEVEL ADJUSTMENT MODE OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3226800

• The ATF level adjustment mode is used for adjusting the ATF level.
• While switching to the ATF level adjustment mode, the P position display of the selector indicator light flashes according to the ATF temperature.

ATF temperature | Selector indicator light (P position display) flashing pattern
--- | ---
High temperature (47 °C {117 °F} or more) |
Appropriate temperature (between 37 °C {99 °F} and under 47 °C {117 °F}) |
Low temperature (less than 37 °C {99 °F}) |  |

• While switching to the ATF level adjustment mode, if the ATF is around the appropriate temperature (between 37 °C {99 °F} and under 47 °C {117 °F}), the TCM performs the idle increase control automatically.
• Verify the ATF level when the ATF temperature is at the appropriate temperature.
• Verify the ATF temperature using the M-MDS or the selector indicator light (P position display) flashing pattern.
• Refer to the Workshop Manual for switching the ATF level adjustment mode.
• If the engine is stopped, the accelerator pedal is depressed, or the vehicle speed is detected, the ATF level adjustment mode is cancelled.