REAR BRAKE (DISC) INSPECTION

id041100800400

Brake Judder Repair Hint

Description

Brake judder concern has the following three characteristics:

Steering wheel vibration

Steering wheel vibrates in the direction of its rotation. This characteristic is most noticeable when applying brakes at a vehicle speed of 100—140 km/h {62—87 mph}.

Floor vibration

When applying brakes, the vehicle body shakes back and forth. The seriousness of shake is not influenced by vehicle speed.

Brake pedal vibration

When applying brakes, a pulsating force tries to push the brake pad back. The pulsation is transmitted to the brake pedal.
The following are the main possible causes of brake judder:

Due to an excessive runout (side-to-side wobble) of disc plate, the thickness of disc plate is uneven.

If the runout is more than 0.05 mm {0.002 in} at the position 10 mm {0.39 in} from the disc plate edge, uneven wear occurs on the disc plate because of uneven pad/plate contact.
If the runout is less than 0.05 mm {0.002 in}, uneven wear does not occur.

The disc plate is deformed by heat.

Repeated panic braking may raise the temperature in some portions of disc plate by approx. 1,000 °C {1,832 °F}. This results in deformed disc plate.

Due to corrosion, the thickness and friction coefficient of disc plate change.

If a vehicle is parked under damp conditions for a long time, corrosion occurs on the friction surface of disc plate.
The thickness of corrosion is uneven and sometimes appears like a wave pattern, which changes the friction coefficient and causes a reaction force.

Inspection and repair procedure

ac9wzw00001872

Lateral runout inspection

1. To secure the disc plate and the hub, tighten the hub nuts upside down or insert a washer (thickness 10 mm {0.39 in}with an inner diameter more than 12 mm {0.47 in}) between the hub bolt and the hub nut.

  Note
  • The component parts of the SST (49 B017 001 or 49 G019 003) can be used as a suitable washer.

2. After tightening all the hub nuts to the same torque, put the dial gauge on the friction surface of disc plate 10 mm {0.39 in} from the disc plate edge.

3. Rotate the disc plate one time and measure the runout.

  Rear disc plate runout limit

  0.05 mm {0.002 in}

Thickness variation inspection

1. Clean the disc plate-to-pad friction surface using a brake cleaner.

2. Measure the points indicated in the illustration using a caliper (micrometer).

3. Subtract the minimum value from the maximum.

  • If the result is not within specification, machine the disc plate using a lathe.

  Thickness variation limit

  0.015 mm {0.0005 in}

  Warning
  • Do not exceed minimum disc plate thickness.

ac9wzw00001873

Disc Plate Thickness Inspection

  Caution
  • Excessive runout may result if the disc plate is removed from the vehicle then machined. Machine the disc plate while installed on the vehicle.

1. Measure the thickness of the disc plate.

  • If the thickness is not within the specification, replace the disc plate.

  Minimum rear disc plate thickness

  16 mm {0.63 in}

  Minimum rear disc plate thickness after machining using a brake lathe on-vehicle

  16.8 mm {0.66 in}

Disc Pad Thickness Inspection

1. Jack up the rear of the vehicle and support it with safety stands.

2. Remove the wheels.

3. Verify the remaining thickness of the pads.

  • Replace the pads as a set: right and left wheels, if either one is at or less than the minimum thickness.

  Minimum rear disc pad thickness

  2.0 mm {0.08 in}

ac9wzw00001874