KEYLESS ENTRY SYSTEM OUTLINE

id091400593700

• All doors lock when the LOCK button on the transmitter is pressed, and unlock when the UNLOCK button is pressed.
• An answer-back function has been adopted which flashes the hazard warning lights when the doors are locked/unlocked using the transmitter.
• An auto-lock function has been adopted which automatically locks the doors if any door is not opened within approx. 30 s after all doors are unlocked by pressing the UNLOCK button on the transmitter.
• A rolling code type transmitter has been adopted to prevent theft by radiowave interception.
• To prevent improper operation while the vehicle is moving, any transmitter button operation is disabled when the ignition is switched to ON.