FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION

id041800816700

1. When removing the right front ABS wheel-speed sensor, perform the following procedure.

  (1) Remove the coolant reserve tank installation bolts and move the coolant reserve tank. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION [MZI-3.7].)

  (2) Remove the power steering reserve tank installation bolt and nut, and move the power steering reserve tank. (See POWER STEERING OIL PUMP REMOVAL/INSTALLATION [L.H.D.].) (See POWER STEERING OIL PUMP REMOVAL/INSTALLATION [R.H.D.].)

2. When removing the left front ABS wheel-speed sensor, perform the following procedure:

  (1) Remove the air cleaner case. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove in the order indicated in the table.

ac9wzw00000145

1 | Front ABS wheel-speed sensor connector
2 | Bolt
3 | Front ABS wheel-speed sensor

4. Install in the reverse order of removal.