TRANSFER OIL SEAL (LH) REPLACEMENT

id031600811500

1. Remove the transfer. (See TRANSFER REMOVAL/INSTALLATION.)

2. Remove the transfer dust seal (LH). (See TRANSFER DUST SEAL (LH) REPLACEMENT.)

3. Insert two tapping screws into the oil seal.

ac9wzw00003175

4. Pry the screws using a fastener remover to remove the oil seal.

ac9wzw00003198

5. Using the SST (49 S034 205) and a hammer, tap a new oil seal until the SST contacts the transfer case.

ac9wzw00003176

  Substitution SST

  • 49 S034 205
  Outer diameter: 67 mm {2.6 in}
  Inner diameter: 59 mm {2.3 in}

6. Install the transfer dust seal (LH). (See TRANSFER DUST SEAL (LH) REPLACEMENT.)

7. Install the transfer. (See TRANSFER REMOVAL/INSTALLATION.)

8. Inspect for leakage of transfer oil.