DTC 11 [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7403500

Description

• Auto leveling control module initial setting

Detection Condition

• Auto leveling system initial setting is not performed or the setting is invalid

Possible Cause

• Auto leveling system initial setting is not performed or the setting is invalid
• Auto leveling control module malfunction

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM AUTO LEVELING SYSTEM INITIAL SETTING • Perform the auto leveling system initial setting. (See AUTO LEVELING SYSTEM INITIALIZATION.) • Perform the headlight auto leveling system DTC inspection. (See DTC INSPECTION [HEADLIGHT AUTO LEVELING SYSTEM].) • Are any DTCs displayed? | Yes | If any DTC other than DTC 11 is displayed • Perform the corresponding DTC inspection first. (See DTC TABLE [HEADLIGHT AUTO LEVELING SYSTEM].) When only DTC 11 is displayed • Replace the auto leveling control module. (See AUTO LEVELING CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.