BREATHER COMPONENT REMOVAL/INSTALLATION [AY6A-EL, AY6AX-EL]

id0517k3296800

1. Disconnect the negative battery cable.

2. Remove the battery. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the battery tray. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

ac9uuw00003904

1 | Clamp
2 | Breather hose cap
3 | Breather hose component
4 | Clamp