PLASTIC PARTS HEAT RESISTING TEMPERATURE [PLASTIC BODY PARTS]

id098011740200

Part Name | Code | Material Name | Heat resisting Temperature °C{°F}
--- | --- | --- | ---
WINDSHIELD MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
COWL GRILLE | PP | POLYPROPYLENE | 95 {203}
FRONT COMBINATION LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 100 {212}
RADIATOR GRILLE | ABS | ABS | 90 {194}
FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
FRONT OVER FENDER | PP | POLYPROPYLENE | 100 {212}
OUTSIDE MIRROR | WITHOUT TURN LIGHT | PANEL | ABS | ABS | 90 {194}
UNDER PANEL | AAS | AAS | 100 {212}
VISOR | AAS | AAS | 100 {212}
WITH TURN LIGHT | PANEL | ABS | ABS | 90 {194}
UNDER PANEL | AAS | AAS | 100 {212}
VISOR | AAS | AAS | 100 {212}
FRONT SIDE GARNISH | PP | POLYPROPYLENE | 100 {212}
SIDE STEP MOLDING | PP | POLYPROPYLENE | 100 {212}
REAR SIDE GARNISH | PP | POLYPROPYLENE | 100 {212}
ROOF MOULDING | AES | AES | 90 {194}
REAR DOOR GARNISH | AES | AES | 90 {194}
REAR OVER FENDER | PP | POLYPROPYLENE | 100 {212}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 100 {212}
HOUSING | AAS | AAS | 100 {212}
LIFTGATE GARNISH | ABS | ABS | 90 {194}
REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
REFLECTOR | LENS | PMMA | ACRYLIC | 100 {212}
HOUSING | AES | AES | 90 {194}
OUTER HANDLE | COLORS | BASE | PC-PET | POLYCARBONATE-PET | 123 {253}
LEVER | PC-PBT | POLYCARBONATE-PBT | 115 {239}
EXCEPT COLORS | BASE | PC-ABS | POLYCARBONATE-ABS | 110 {230}
LEVER | PC-ABS | POLYCARBONATE-ABS | 110 {230}
HIGH-MOUNT BRAKE LIGHT | LENS | PMMA | ACRYLIC | 100 {212}
HOUSING | ABS | ABS | 94 {201}
REAR SPOILER | PC-PET | POLYCARBONATE-PET | 140 {284}
SHROUD PANEL | PP | POLYPROPYLENE | 100 {212}

  Note
  • The application of temperatures higher than heat resisting temperatures may result in part deformation.