DTC U3000:01 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3393200

Description | Electrical malfunction inside BSM control module
--- | ---
Detection condition | • BSM control module is detected an electrical malfunction inside.
Fail-safe function | • Blind spot monitoring (BSM) system is stopped.
Possible cause | • BSM control module malfunction
System wiring diagram | Not applicable

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM DTC INSPECTION AND VERIFY BSM CONTROL MODULE MALFUNCTION • Clear the DTC for the BSM control module using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Retrieve the BSM control module DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Is the same DTC displayed? | Yes | Replace the BSM control module, then go to the next step. (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
No | Go to the next step.
2 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
No | DTC troubleshooting completed.