ON-BOARD DIAGNOSTIC SYSTEM EXTERNAL TESTER COMMUNICATION FUNCTION [AY6A-EL, AY6AX-EL]

id0502k1280500

• The on-board diagnostic system external tester communication function enables sending/receiving of data between modules and an external tester.
• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been adopted.
• A connector shape and 16-pin terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this DLC-2.

am5ezn00001698

Terminal | Function
--- | ---
A | Battery power supply terminal
B | -
C | -
D | -
E | HS-CAN-use Lo terminal
F | HS-CAN-use Hi terminal
G | -
H | Serial communication GND terminal
I | -
J | Body GND terminal
K | MS-CAN-use Lo terminal
L | MS-CAN-use Hi terminal
M | -
N | -
O | -
P | -