PARKING SENSOR SWITCH/INDICATOR REMOVAL/INSTALLATION

id092200023700

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the bonnet release lever. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

4. Pull the parking sensor switch/indicator in the direction of the arrow (2) shown in the figure while pressing the tab in the direction of the arrow (1) shown in the figure, detach the tab and lower panel, and then remove the parking sensor switch/indicator from the lower panel.

ac9wzw00002628

5. Disconnect the connector.

6. Install in the reverse order of removal.