REAR AUTO LEVELING SENSOR INSPECTION

id091800806800

1. Disconnect the negative battery cable.

2. Jack up the vehicle.

3. Remove the wheels and tire (LH). (See GENERAL PROCEDURES (SUSPENSION).)

4. Remove the rear auto leveling sensor. (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

5. Connect three 1.5 V dry cell batteries in a series.

ac9wzw00001276

6. Connect the positive pole of the battery to rear auto leveling sensor terminal C, and the negative pole to terminal A, then apply voltage of 4.5 V between terminals C and A.

7. Connect the tester as shown in the figure.

8. Measure the voltage while the link is moved up and down slowly.

acxwzw00000841

  • If not as indicated in the table, replace the rear auto leveling sensor.