INTERLOCK CABLE INSPECTION

id051800800200

1. Turn the ignition switch to the ON position. (Engine off)

2. Remove the clip of the selector lever base plate, then remove the interlock cable from the U-groove.

L.H.D.

ac9wzw00000601

R.H.D.

ac9wzw00000602

3. Remove the interlock cable from the selector lever.

4. Verify that the interlock cable moves freely with the brake pedal depressed.

ac9uuw00002009

  • If there is any malfunction, inspect the interlock cable for abnormal winding. If any abnormal winding found, correct it.
  • If the malfunction persists after correcting the interlock cable winding, replace it.