DTC INSPECTION [AUTO LIGHT/WIPER CONTROL MODULE]

id0902j1345400

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “LCM”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

4. After completion of repairs, clear all DTCs stored in the auto light/wiper control module. (See CLEARING DTC [AUTO LIGHT/WIPER CONTROL MODULE].)