FRONT DOOR CHECKER REMOVAL/INSTALLATION

id091100520400

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00003062

1 | Bolt A
2 | Bolt B
3 | Front door checker
4 | Front door

4. Install in the reverse order of removal.