A/C COMPRESSOR REMOVAL/INSTALLATION

id071100801000

1. Disconnect the negative battery cable.

2. Discharge the refrigerant. (See REFRIGERANT CHARGING.)

3. Remove the drive belt. (See DRIVE BELT REMOVAL/INSTALLATION [MZI-3.7].)

4. Remove the front cooler hose (HI). (See REFRIGERANT LINE REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table. Do not allow compressor oil to spill.

  Caution
  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise or other malfunction could occur. Always plug open fittings immediately after removing any refrigeration cycle parts.

ac9uuw00000956

1 | Front cooler hose (LO) (See REFRIGERANT LINE REMOVAL/INSTALLATION.)
2 | Front cooler pipe No.2 (See REFRIGERANT LINE REMOVAL/INSTALLATION.)
3 | A/C compressor connector
4 | A/C compressor (See A/C Compressor Installation Note (1).) (See A/C Compressor Installation Note (2).)

6. Install in the reverse order of removal.

7. Perform the refrigerant system performance test. (See REFRIGERANT SYSTEM PERFORMANCE TEST.)

A/C Compressor Installation Note (1)

  Caution
  • Due to the high moisture-absorption characteristics of the compressor oil, it may absorb moisture if left over a long period of time thereby negatively affecting A/C operation. Drain the compressor oil and refill within 10 min. of each other.

1. Rotate new A/C compressor shaft six to eight revolutions while collecting refrigerant oil in a clean measuring device. Use this refrigerant oil to refill new compressor. Do not allow refrigerant oil to become contaminated.

2. Rotate old A/C compressor shaft six to eight revolutions while collecting refrigerant oil in a separate, clean measuring device.

3. Compare those oil amounts. The amount of the oil drained from the new A/C compressor should be greater than the old one.

4. Pour the same amount oil of drained from the old A/C compressor back into the new A/C compressor.

am8rrw00000755

  A/C compressor oil type

  • DENSO OIL8

  A/C compressor oil sealed volume (approx. quantity)

  • 160 ml {160 cc, 5.41 fl oz}

A/C Compressor Installation Note (2)

1. After replacing the A/C compressor, add compressor oil to the refrigeration cycle.