FRONT DOOR LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

id091400800400

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Front door module (See FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00002308

1 | Connector
2 | Screw A
3 | Screw B
4 | Front door latch and lock actuator

4. Install in the reverse order of removal.