IGNITION COIL INSPECTION [MZI-3.7]

id0118c2800300

Secondary Coil Resistance Inspection

1. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [MZI-3.7].)

2. Using a tester, measure the resistance between the ignition coil terminal A and ignition coil boot socket.

ac9wzw00002114

  • If not within the specification, replace the ignition coil.

  Ignition coil secondary coil resistance

  5—6 kilohms