FRONT TURN LIGHT BULB REMOVAL/INSTALLATION

id091800805000

1. Disconnect the negative battery cable.

2. When removing the front turn light bulb on the right side, remove the coolant reserve tank first. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove in the order indicated in the table.

ac9wzw00002568

1 | Socket
2 | Front turn light bulb

4. Install in the reverse order of removal.