FRONT FOG LIGHT BULB REMOVAL/INSTALLATION

id091800802300

1. Disconnect the negative battery cable.

2. Remove the front under cover B. (See FRONT UNDER COVER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00002564

1 | Connector
2 | Front fog light bulb (See Front Fog Light Bulb Removal Note.)

4. Install in the reverse order of removal.

Front Fog Light Bulb Removal Note

1. Remove the front fog light bulb by turning it in the direction shown by the arrow.

ac9uuw00000503

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When handling the bulb, hold the flange, not the glass.