RUNNING LIGHT SYSTEM OPERATION

id091800103000

• The following table indicates the running light operation specification.

IG | Parking brake | Light switch | Dimmer switch | Running light
--- | --- | --- | --- | ---
ON | Released | AUTO*1 | LOW | ON
HIGH | ON
PASS | ON
OFF | LOW | ON
HIGH | ON
PASS | ON
TNS | LOW | OFF
HIGH | OFF
PASS | OFF
HEAD | LOW | OFF
HIGH | OFF
PASS | OFF

*1 :If the auto light sensor detects that the TNS and headlights are off when the light switch is in the AUTO position, the running light illuminates.