REAR WIPER AND WASHER SWITCH INSPECTION

id091900800400

1. Disconnect the negative battery cable.

2. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove the wiper and washer switch. (See WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the windshield wiper and washer switch is as indicated in the table.

  • If not as indicated in the table, replace the wiper and washer switch. (See WINDSHIELD WIPER AND WASHER SWITCH REMOVAL/INSTALLATION.)

Wiper And Washer Switch LH Side

acxaaw00000688

acxaaw00000689

Wiper And Washer Switch RH Side

acxaaw00001032

ac9wzw00001210