FRONT STABILIZER REMOVAL/INSTALLATION [L.H.D.]

id0213008004b1

  Caution
  • Secure the steering wheel using tape or a cable to prevent the steering shaft from rotating after disconnecting the steering shaft. If the steering wheel rotates after the steering shaft and the steering gear and linkage are disconnected, the internal parts of the clock spring could be damaged.

1. Drain the power steering fluid. (See POWER STEERING FLUID INSPECTION.)

2. Remove the front under cover A and front under cover B. (See FRONT UNDER COVER REMOVAL/INSTALLATION.)

3. Disconnect the front auto leveling sensor connector. (Vehicle with headlight auto leveling system) (See FRONT AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

4. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

5. Remove the transverse member. (See TRANSVERSE MEMBER REMOVAL/INSTALLATION.)

6. Remove the intermediate shaft installation bolt, and disconnect the steering shaft. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

7. Remove the front crossmember component. (See FRONT CROSSMEMBER REMOVAL/INSTALLATION [L.H.D.].)

8. Remove in the order indicated in the table.

9. Install in the reverse order of removal.

10. Inspect for front wheel alignment, and adjust it as necessary. (See FRONT WHEEL ALIGNMENT.)

ac9uuw00001926

1 | Front stabilizer component
2 | Front stabilizer control link
3 | Stabilizer bracket (See Stabilizer Bracket Installation Note.)
4 | Stabilizer bushing (See Stabilizer Bushing Installation Note.)
5 | Front stabilizer (See Front Stabilizer Installation Note.)

Front Stabilizer Installation Note

1. Install the stabilizer bar so that the identification mark is on the left side of the vehicle.

ac9uuw00002069

Stabilizer Bushing Installation Note

1. Align the outer side of the positioning plate with the stabilizer bushing.

am8rrw00001822

Stabilizer Bracket Installation Note

1. Install the stabilizer bracket so that the arrow is pointed to the front.

ampjjw00000547