AIRFLOW MODE CONTROL OPERATION

id074000102900

Airflow Mode Automatic Control

Front

  • The front climate control unit determines the front mode actuator opening angle based on the target temperature.

ac9uun00000232

Rear

  • When the rear control switch is off, the rear airflow mode control determines the rear mode actuator opening angle using the target temperature for the rear which is calculated by the front climate control unit based on the set temperature which has been set using the driver-side temperature setting dial.
  • When the rear control switch is on, the rear airflow mode control determines the rear mode actuator opening angle using the rear target temperature which is calculated by the front climate control unit based on the set temperature which has been set using the rear temperature setting dial.

ac9wzn00000511

Correction

Warm-up correction

  • Switches the airflow mode after the engine is started in winter in accordance with the increase in engine coolant temperature to prevent discomfort caused by cold air blown towards the feet.

  ac9wzn00000610

MAX HOT and MAX COLD correction

  Front

  • When the set temperature is at 32.0 or 15.0, the airflow mode is set as shown in the table.

TEMPERATURE CONTROL DIAL | AIRFLOW MODE
--- | ---
DRIVER SIDE | PASSENGER SIDE
15.0 | 15.0 | VENT
15.0 | EXCEPT 15.0, 32.0 | VENT
EXCEPT 15.0, 32.0 | 15.0 | VENT
15.0 | 32.0 | BI-LEVEL
32.0 | 15.0 | BI-LEVEL
32.0 | EXCEPT 15.0, 32.0 | HEAT
EXCEPT 15.0, 32.0 | 32.0 | HEAT
32.0 | 32.0 | HEAT

  Rear

  • The airflow mode is fixed in heat with the set temperature of 32.0 (MAX HOT), and in vent with 15.0 (MAX COLD).

Airflow Mode Manual Control

• The airflow modes can be switched by operating the airflow mode selector switch and the front defroster switch.

FRONT | VENT, BI-LEVEL, HEAT, HEAT/DEF, DEFROSTER