AUTO LEVELING CONTROL MODULE REMOVAL/INSTALLATION

id091800805500

L.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

  (3) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00001261

4. Remove the nut.

5. Remove the auto leveling control module.

6. Install in the reverse order of removal.

7. Perform the auto leveling system initialization. (See AUTO LEVELING SYSTEM INITIALIZATION.)

R.H.D.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

  (3) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00001262

4. Remove the bolt.

5. Remove the auto leveling control module.

6. Install in the reverse order of removal.

7. Perform the auto leveling system initialization. (See AUTO LEVELING SYSTEM INITIALIZATION.)