FRONT SEAT REMOVAL/INSTALLATION

id091300800200

  Warning
  • Handling the front seats improperly can accidentally deploy the side air bag, which may seriously injure you. Read air bag system service warnings and cautions before handling the front seats. (See AIR BAG SYSTEM SERVICE WARNINGS) (See AIR BAG SYSTEM SERVICE CAUTIONS)

  Caution
  • After removing a front seat, do not operate the slider lever. If the slider lever is operated, the left and right slide positions will deviate, and the slide adjuster may be damaged after the front seat is installed.
  • Verify that there are no malfunctions in the sliding mechanism after installing a front seat.
  • When performing the procedure with a front seat removed from the vehicle, perform the procedure on a clean rag so as not to damage or soil the seat.

Driver side seat

1. Switch the ignition to off.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the negative battery cable and wait 1 min. or more.

4. Remove in the order indicated in the table.

ac9wzw00002468

1 | Cover
2 | Bolt
3 | Connector
4 | Front seat

5. Install in the reverse order of removal.

Passenger side seat

Vehicles with power seat system (Type A)

1. Switch the ignition to off.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the negative battery cable and wait 1 min. or more.

4. Remove in the order indicated in the table.

ac9wzw00002471

1 | Cover
2 | Bolt
3 | Connector
4 | Front seat

5. Install in the reverse order of removal.

Vehicles with power seat system (Type B)

1. Switch the ignition to off.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the negative battery cable and wait 1 min. or more.

4. Pull the front seat belt lower anchor cover in the direction of arrow shown in the figure, while detaching the hooks A.

ac9wzw00002469

5. Move the front seat belt lower anchor cover in the direction of arrow shown in the figure, then detaching the hooks B.

ac9wzw00002470

6. Remove the front seat belt lower anchor. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

7. Remove in the order indicated in the table.

ac9wzw00001287

1 | Cover
2 | Bolt
3 | Connector
4 | Front seat

8. Install in the reverse order of removal.

Vehicles without power seat system

1. Switch the ignition to off.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the negative battery cable and wait 1 min. or more.

4. Remove in the order indicated in the table.

ac9wzw00002467

1 | Cover
2 | Bolt
3 | Connector
4 | Front seat

5. Install in the reverse order of removal.