LIFTGATE OUTER HANDLE REMOVAL/INSTALLATION

id091400803700

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove the rear finisher. (See REAR FINISHER REMOVAL/INSTALLATION.)

6. Disconnect the liftgate outer handle switch connector. (Vehicles with power liftgate system)

7. Disconnect the cable. (Vehicles without power liftgate system)

8. Remove in the order indicated in the table.

ac9uuw00002397

1 | Nut
2 | Liftgate outer handle

9. Install in the reverse order of removal.