FRONT SEAT SLIDE ADJUSTER REMOVAL/INSTALLATION

id091300956700

  Caution
  • After removing a front seat, do not operate the slider lever. If the slider lever is operated, the left and right slide positions will deviate, and the slide adjuster may be damaged after the front seat is installed.
  • Verify that there are no malfunctions in the sliding mechanism after installing a front seat.
  • When performing the procedure with a front seat removed from the vehicle, perform the procedure on a clean rag so as not to damage or soil the seat.

1. Disconnect the negative battery cable and wait 1 min or more.

2. Remove the following parts:

  (1) Front seat (See FRONT SEAT REMOVAL/INSTALLATION.)

  (2) Front seat side cover (See FRONT SEAT SIDE COVER REMOVAL/INSTALLATION.)

  (3) Front seat front cover (See FRONT SEAT FRONT COVER REMOVAL/INSTALLATION.)

  (4) Front seat cushion (See FRONT SEAT CUSHION TRIM REMOVAL/INSTALLATION.)

  (5) Front seat back component (See FRONT SEAT BACK COMPONENT REMOVAL/INSTALLATION.)

3. Install in the reverse order of removal.