EXTERIOR OPEN/CLOSE FUNCTION OUTLINE

id091200102000

• A exterior open/close function has been adopted so that the power window system can be operated from outside the vehicle.
• This system can operate in conjunction with the following:

  ― Transmitter
  ― Front side request switch (with advanced keyless system, close operation only)

• An automatic reverse function operates if the door glass is obstructed during close operation.

Operation item | Open operation (Manual open) | Close operation (Manual close)
--- | --- | ---
Transmitter | UNLOCK button operation (hold, approx. 2.5 s or more) | LOCK operation (hold, approx. 2.5 s or more)
Request switch (With advanced keyless system) | — | Long press, approx. 1.5 s or more