PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

id081000801900

  Warning
  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the air bag system service warnings and cautions before handling the air bag module. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)

1. Turn the ignition switch to the OFF position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Front scuff plate inner (Passenger side) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Front side trim (Passenger side) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (8) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (9) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (10) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (11) Dashboard garnish (See DASHBOARD GARNISH REMOVAL/INSTALLATION.)

4. Remove the bolts.

L.H.D.

ac9wzw00000939

R.H.D.

ac9wzw00000940

5. Remove the screws.

6. Remove the clips.

7. Remove the connector.

8. Remove the passenger-side air bag module in the direction of the arrow

9. Install in the reverse order of removal.

10. Turn the ignition switch to the ON position.

11. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system. (See FLOWCHART.)