COMBINATION SWITCH REMOVAL/INSTALLATION

id091800802500

  Warning
  • If the negative battery cable or the steering angle sensor connector is disconnected, the stored initial position of the steering angle sensor will be cleared and the DSC will not operate properly, making the vehicle unsafe to drive. Perform the steering angle sensor initialization procedure after connecting the negative battery cable.

1. Turn the ignition switch to the OFF position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove the following parts:

  (1) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (2) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (3) Lower column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

4. Put aside the upper column cover.

5. Remove in the order indicated in the table.

ac9wzw00001412

1 | Connector
2 | Screw
3 | Combination switch

6. Disconnect the steering angle sensor connector.

7. Install in the reverse order of removal.