FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

id091800800700

  Warning
  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

  Note
  • Fogging or condensation on the inside of the front combination lights may occur due to a natural phenomenon occurring as a result of a temperature difference between the interior and exterior of the combination lights. However, it has no effect on the light performance because the temperature inside the front combination lights rises after illuminating the headlights or a period of time has elapsed.

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00002595

4. While pressing the clip tab in the direction of the arrows (1) shown in the figure, press the clip in the direction of the arrow (2) shown in the figure to detach the clip tab and front combination light.

ac9wzw00002602

5. Remove the clip.

6. Remove the bolts.

ac9wzw00002596

7. Remove the protector.

8. Remove the bolts.

ac9wzw00002597

9. Remove the fastener.

ac9wzw00002598

10. Pull the front combination light in the direction of the arrow shown in the figure and pull out the front combination light pin from the body.

ac9wzw00002599

11. Remove the front combination light.

12. Install in the reverse order of removal.(See Front combination light installation note.)

13. Adjust the headlight aiming. (See HEADLIGHT AIMING.)

Front combination light installation note

  Caution
  • When replacing the front combination light, refer to the following disassembly figure and verify that parts are assembled correctly. If a part has not been assembled correctly, it could cause problems such as water leakage or fogging in the housing.

Halogen type

ac9wzw00003292

Discharge type

ac9wzw00003293

  Note
  • Parts necessary for assembly vary depending on the vehicle's manufacturing period and specifications.