ULTRASONIC SENSOR SHORT-CORD INSPECTION

id092200037000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Rear combination light (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

  (2) Rear bumper (See REAR BUMPER REMOVAL/INSTALLATION.)

  (3) Rear reflector (See REAR BUMPER DISASSEMBLY/ASSEMBLY.)

  (4) Ultrasonic sensor short-cord (See ULTRASONIC SENSOR SHORT-CORD REMOVAL/INSTALLATION.)

3. Verify that the continuity between the ultrasonic sensor short-cord terminals is as indicated in the table.

ac9wzw00002680

ac9wzw00002681

  • If not as indicated in the table, replace the ultrasonic sensor short-cord.