IGNITION COIL REMOVAL/INSTALLATION [MZI-3.7]

id0118c2800200

1. Disconnect the negative battery cable.

2. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

4. Remove in the order indicated in the table.

  Caution
  • Apply small amount of the specified dielectric grease to the inside of the ignition coils, then install the ignition coils to the spark plugs.
    ― Specified grease: Motorcraft XG-3A

5. Install in the reverse order of removal.

ac9wzw00002113

1 | Connector
2 | Ignition coil