DTC U3000:01 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0902q2393200

Description | BSM control module internal electrical malfunction
--- | ---
Detection condition | • BSM control module detects the internal electrical malfunction.
Possible cause | • BSM control module malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM DTC INSPECTION AND VERIFY BSM CONTROL MODULE MALFUNCTION • Clear the DTC for the BSM control module using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Retrieve the BSM control module DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) • Is the same DTC displayed? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the BSM control module. (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].) Go to the next step.
No | Go to the next step.
2 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE].)
No | DTC troubleshooting completed.