LIFTGATE LATCH AND LOCK ACTUATOR INSPECTION

id091400810200

Vehicles With PLG

Liftgate latch switch

1. When inspecting the latch, press the latch lever using a flathead screwdriver or a similar tool.

am8rrw00000485

2. Verify that the continuity is as indicated in the table.

ac9uuw00002401

  • If not as indicated in the table, replace the liftgate latch and lock actuator.

  ac9uuw00002402

Full latch switch, Half latch switch, Return switch

1. Press the latch in using a flathead screwdriver to inspect the latch condition.

am8rrw00000489

2. Verify that the continuity is as indicated in the table.

ac9wzw00001919

  • If not as indicated in the table, replace the liftgate latch and lock actuator.

  ac9uuw00002352

Closer motor

1. Apply battery positive voltage and connect ground to the corresponding closer motor terminals, and inspect the closer motor operation.

ac9uuw00002403

ac9uuw00002409

  • If not as indicated in the table, replace the liftgate latch and lock actuator.

Operation | Terminal
--- | ---
A | B
Normal rotation | GND | B+
Reverse rotation | B+ | GND

Vehicles Without PLG

Liftgate latch switch

1. When inspecting the latch, press the latch lever using a flathead screwdriver or a similar tool.

am8rrw00000485

2. Verify that the continuity is as indicated in the table.

ac9uuw00002401

  • If not as indicated in the table, replace the liftgate latch and lock actuator.

ac9uuw00002402

Liftgate lock actuator

1. Apply battery positive voltage and connect ground to the corresponding liftgate lock actuator terminals, and inspect the liftgate lock actuator operation.

ac9uuw00002404

  • If not as specified, replace the liftgate latch and lock actuator.

Operation | Terminal
--- | ---
A | B
Lock | B+ | GND
Unlock | GND | B+