ADVANCED KEY ID CODE REGISTRATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914005158z6

  Caution
  • Do not place the following devices in the vehicle while programming, otherwise programming cannot be performed.
    ― M-MDS
    ― Personal computer
    ― Device that can send/receive radio waves
  • Verify that the other transmitter is not being operated around the servicing area during advanced key programming.

  Note
  • Use the M-MDS and start programming if the condition corresponds to the following:
    ― One or No Programmed Advanced Keys
    ― Keyless control module is replaced
  • If six advanced keys are already programmed, the programming mode does not activate. If programming is needed, use the M-MDS to erase the unnecessary advanced key programming.

With two programmed advanced keys

1. Bring the programmed advanced keys (2) and a unprogrammed advanced key into the vehicle.

2. Close all doors.

3. Insert the supplementary key into the ignition key cylinder.

  Note
  • Complete the procedures up to Step 7 within 30 s after the supplementary key is inserted.

4. Turn the ignition switch to the ON position.

5. Press the UNLOCK button on advanced key 1.

6. Press the UNLOCK button on advanced key 2.

7. From the ignition switch in the ON position, switch the ignition switch in the order indicated below.

  ― ACC→ON→ACC→ON→ACC→ON

8. Open the driver-side front door, press the door switch twice, and then close the door.

  Note
  • After Step 8 is completed and the advanced key programming mode is activated, the door lock actuator operates to lock, and then operates to unlock.
  • If the door lock actuator does not operate, repeat the procedure from Step 2.

9. Press the UNLOCK button on the unprogrammed advanced key twice.

  Note
  • After Step 9 is completed and the advanced key is programmed, the door lock actuator operates to lock, and then operates to unlock.

10. If programming more advanced keys, remove the supplementary key once, and then repeat the procedure from Step 2.

Using M-MDS

1. Fully lower the driver-side door glass.

2. Connect the M-MDS to the DLC-2.

ac9uuw00000452

3. Pull out the M-MDS cable from the door glass opening and set the M-MDS outside the vehicle.

  Caution
  • Protect the cable and body contact area with a clean rag, otherwise they could be damaged.

4. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Body”.
  2. Select “Security”.

5. Then, select items from the screen menu in the following order.

  1. Select “PATS Functions”.
  2. Select “Program Additional card key”.

6. Security access begins and the M-MDS displays the “OUT-CODE“.

  Note
  • When “OUT-CODE” is first displayed, turning the ignition switch from the OFF to the ON position 5 times will change the “OUT-CODE”.

7. Input the “IN-CODE” that corresponds to the “OUT-CODE” displayed on the M-MDS screen.

  Note
  • After Step 7 is completed and the advanced key programming is activated, the door lock actuator operates to lock, and then operates to unlock.

8. Press the unprogrammed advanced key UNLOCK button twice.

  Note
  • After Step 8 is completed and the advanced key is programmed, the door lock actuator operates to lock, and then operates to unlock.

9. If additional advanced keys are to be programmed, go to the additional advanced key programming mode according to the instructions on the M-MDS or equivalent screen.